|  |  |
| --- | --- |
| **VLAN** | **Subnet** |
| 2 (Accounting) | 192.168.2.0/24 |
| 3(Financial) | 192.168.3.0/24 |
| 4(Human\_Resources) | 192.168.4.0/24 |
| 5(IT\_Department) | 192.168.5.0/24 |
| 6(Management) | 192.168.6.0/24 |
| 7(Servers) | 192.168.7.0/24 |
| 999(Nonexistent VLAN) |  |
|  |  |

Gateways – every first address of a subnet. For HSRP/VRRP virtual address – every second.

192.168.x.3 – 50 Reserved for static addresses

192.168.x.51-254 Reserved for DHCP assigning for the clients

192.168.10.0/24 – for point-to-point /31 L3 links